**CalAdvocates Data Request 3.4**

**Section 8.2, Vegetation Management and Inspections, of PacifiCorp’s 2025 WMP Update -** For Table 8-19, Vegetation Management QA/QC Program:

1. Please justify why a 10% sample size for Pole Clearing is a sufficient sample size for the purpose of QA/QC.
2. What is PacifiCorp’s procedural response to programs that do not meet the yearly target pass rate?

**Response to CalAdvocates Data Request 3.4**

1. Typically, 10 percent is the minimum sample size per circuit for a pole clearing audit. Poles cleared are also reviewed during post audit of annual corrective work for distribution identified during patrol inspections (target 100 percent post audit) and the Company is working on a process to record these reviews during other post audit activities.
2. PacifiCorp reviews audit findings with vegetation contractors during the normal course of business to identify opportunities for improvement. PacifiCorp also has developed key performance indicators, which includes number of audit findings, and reviews these with the vegetation management contractors typically on a quarterly basis.